0 10 20 30 40 50 60 70 80 90 100 0 50 100 150 200 250 300 350

Frame

Number of Streamlines number of the streamlines reused from the previous frame using the temporally coherent seeding strategy number of the streamlines advected in the current frame using the temporally coherent seeding strategy number of the streamlines present in the current frame using the temporally coherent seeding strategy number of the streamlines present (advected) in the current frame using the temporally incoherent seeding strategy